| LCD Library 1.2.1 LCD Library - LCD control class hierarchy library. Drop in replacement for the LiquidCrystal Library.

- Main Page
- Classes
- Files

- File List
- File Members

/Users/fmalpartida/development/ardWorkspace/LiquidCrystal_I2C/LiquiCrystal_I2C/LiquidCrystal_I2C.cpp
Go to the documentation of this file.

    00001 // ---------------------------------------------------------------------------
    00002 // Created by Francisco Malpartida on 20/08/11.
    00003 // Copyright 2011 - Under creative commons license 3.0:
    00004 //        Attribution-ShareAlike CC BY-SA
    00005 //
    00006 // This software is furnished "as is", without technical support, and with no
    00007 // warranty, express or implied, as to its usefulness for any purpose.
    00008 //
    00009 // Thread Safe: No
    00010 // Extendable: Yes
    00011 //
    00012 // @file LiquidCrystal_I2C.c
    00013 // This file implements a basic liquid crystal library that comes as standard
    00014 // in the Arduino SDK but using an I2C IO extension board.
    00015 //
    00016 // @brief
    00017 // This is a basic implementation of the LiquidCrystal library of the
    00018 // Arduino SDK. The original library has been reworked in such a way that
    00019 // this class implements the all methods to command an LCD based
    00020 // on the Hitachi HD44780 and compatible chipsets using I2C extension
    00021 // backpacks such as the I2CLCDextraIO with the PCF8574* I2C IO Expander ASIC.
    00022 //
    00023 // The functionality provided by this class and its base class is identical
    00024 // to the original functionality of the Arduino LiquidCrystal library.
    00025 //
    00026 //
    00027 //
    00028 // @author F. Malpartida - fmalpartida@gmail.com
    00029 // ---------------------------------------------------------------------------
    00030 #if (ARDUINO <  100)
    00031 #include <WProgram.h>
    00032 #else
    00033 #include <Arduino.h>
    00034 #endif
    00035 #include <inttypes.h>
    00036 #include "I2CIO.h"
    00037 #include "LiquidCrystal_I2C.h"
    00038
    00039 // CONSTANT  definitions
    00040 // ---------------------------------------------------------------------------
    00041
    00042 // flags for backlight control
    00048 #define LCD_NOBACKLIGHT 0x00
    00049
    00055 #define LCD_BACKLIGHT   0xFF
    00056
    00057
    00058 // Default library configuration parameters used by class constructor with
    00059 // only the I2C address field.
    00060 // ---------------------------------------------------------------------------
    00066 #define EN 6  // Enable bit
    00067
    00073 #define RW 5  // Read/Write bit
    00074
    00080 #define RS 4  // Register select bit
    00081
    00088 #define D4 0
    00089 #define D5 1
    00090 #define D6 2
    00091 #define D7 3
    00092
    00093
    00094 // CONSTRUCTORS
    00095 // ---------------------------------------------------------------------------
    00096 LiquidCrystal_I2C::LiquidCrystal_I2C( uint8_t lcd_Addr )
    00097 {
    00098    config(lcd_Addr, EN, RW, RS, D4, D5, D6, D7);
    00099 }
    00100
    00101
    00102 LiquidCrystal_I2C::LiquidCrystal_I2C(uint8_t lcd_Addr, uint8_t backlighPin,
    00103                                      t_backlighPol pol = POSITIVE)
    00104 {
    00105    config(lcd_Addr, EN, RW, RS, D4, D5, D6, D7);
    00106    setBacklightPin(backlighPin, pol);
    00107 }
    00108
    00109 LiquidCrystal_I2C::LiquidCrystal_I2C(uint8_t lcd_Addr, uint8_t En, uint8_t Rw,
    00110                                      uint8_t Rs)
    00111 {
    00112    config(lcd_Addr, En, Rw, Rs, D4, D5, D6, D7);
    00113 }
    00114
    00115 LiquidCrystal_I2C::LiquidCrystal_I2C(uint8_t lcd_Addr, uint8_t En, uint8_t Rw,
    00116                                      uint8_t Rs, uint8_t backlighPin,
    00117                                      t_backlighPol pol = POSITIVE)
    00118 {
    00119    config(lcd_Addr, En, Rw, Rs, D4, D5, D6, D7);
    00120    setBacklightPin(backlighPin, pol);
    00121 }
    00122
    00123 LiquidCrystal_I2C::LiquidCrystal_I2C(uint8_t lcd_Addr, uint8_t En, uint8_t Rw,
    00124                                      uint8_t Rs, uint8_t d4, uint8_t d5,
    00125                                      uint8_t d6, uint8_t d7 )
    00126 {
    00127    config(lcd_Addr, En, Rw, Rs, d4, d5, d6, d7);
    00128 }
    00129
    00130 LiquidCrystal_I2C::LiquidCrystal_I2C(uint8_t lcd_Addr, uint8_t En, uint8_t Rw,
    00131                                      uint8_t Rs, uint8_t d4, uint8_t d5,
    00132                                      uint8_t d6, uint8_t d7, uint8_t backlighPin,
    00133                                      t_backlighPol pol = POSITIVE )
    00134 {
    00135    config(lcd_Addr, En, Rw, Rs, d4, d5, d6, d7);
    00136    setBacklightPin(backlighPin, pol);
    00137 }
    00138
    00139 // PUBLIC METHODS
    00140 // ---------------------------------------------------------------------------
    00141
    00142 //
    00143 // begin
    00144 void LiquidCrystal_I2C::begin(uint8_t cols, uint8_t lines, uint8_t dotsize)
    00145 {
    00146
    00147    init();     // Initialise the I2C expander interface
    00148    LCD::begin ( cols, lines, dotsize );
    00149 }
    00150
    00151
    00152 // User commands - users can expand this section
    00153 //----------------------------------------------------------------------------
    00154 // Turn the (optional) backlight off/on
    00155
    00156 //
    00157 // setBacklightPin
    00158 void LiquidCrystal_I2C::setBacklightPin ( uint8_t value, t_backlighPol pol = POSITIVE )
    00159 {
    00160    _backlightPinMask = ( 1 << value );
    00161    _polarity = pol;
    00162    setBacklight(BACKLIGHT_OFF);
    00163 }
    00164
    00165 //
    00166 // setBacklight
    00167 void LiquidCrystal_I2C::setBacklight( uint8_t value )
    00168 {
    00169    // Check if backlight is available
    00170    // ----------------------------------------------------
    00171    if ( _backlightPinMask != 0x0 )
    00172    {
    00173       // Check for polarity to configure mask accordingly
    00174       // ----------------------------------------------------------
    00175       if  (((_polarity == POSITIVE) && (value > 0)) ||
    00176            ((_polarity == NEGATIVE ) && ( value == 0 )))
    00177       {
    00178          _backlightStsMask = _backlightPinMask & LCD_BACKLIGHT;
    00179       }
    00180       else
    00181       {
    00182          _backlightStsMask = _backlightPinMask & LCD_NOBACKLIGHT;
    00183       }
    00184       _i2cio.write( _backlightStsMask );
    00185    }
    00186 }
    00187
    00188
    00189 // PRIVATE METHODS
    00190 // ---------------------------------------------------------------------------
    00191
    00192 //
    00193 // init
    00194 int LiquidCrystal_I2C::init()
    00195 {
    00196    int status = 0;
    00197
    00198    // initialize the backpack IO expander
    00199    // and display functions.
    00200    // ------------------------------------------------------------------------
    00201    if ( _i2cio.begin ( _Addr ) == 1 )
    00202    {
    00203       _i2cio.portMode ( OUTPUT );  // Set the entire IO extender to OUTPUT
    00204       _displayfunction = LCD_4BITMODE | LCD_1LINE | LCD_5x8DOTS;
    00205       status = 1;
    00206       _i2cio.write(0);  // Set the entire port to LOW
    00207    }
    00208    return ( status );
    00209 }
    00210
    00211 //
    00212 // config
    00213 void LiquidCrystal_I2C::config (uint8_t lcd_Addr, uint8_t En, uint8_t Rw, uint8_t Rs,
    00214                                 uint8_t d4, uint8_t d5, uint8_t d6, uint8_t d7 )
    00215 {
    00216    _Addr = lcd_Addr;
    00217
    00218    _backlightPinMask = 0;
    00219    _backlightStsMask = LCD_NOBACKLIGHT;
    00220    _polarity = POSITIVE;
    00221
    00222    _En = ( 1 << En );
    00223    _Rw = ( 1 << Rw );
    00224    _Rs = ( 1 << Rs );
    00225
    00226    // Initialise pin mapping
    00227    _data_pins[0] = ( 1 << d4 );
    00228    _data_pins[1] = ( 1 << d5 );
    00229    _data_pins[2] = ( 1 << d6 );
    00230    _data_pins[3] = ( 1 << d7 );
    00231 }
    00232
    00233
    00234
    00235 // low level data pushing commands
    00236 //----------------------------------------------------------------------------
    00237
    00238 //
    00239 // send - write either command or data
    00240 void LiquidCrystal_I2C::send(uint8_t value, uint8_t mode)
    00241 {
    00242    // No need to use the delay routines since the time taken to write takes
    00243    // longer that what is needed both for toggling and enable pin an to execute
    00244    // the command.
    00245
    00246    if ( mode == FOUR_BITS )
    00247    {
    00248       write4bits( (value & 0x0F), COMMAND );
    00249    }
    00250    else
    00251    {
    00252       write4bits( (value >> 4), mode );
    00253       write4bits( (value & 0x0F), mode);
    00254    }
    00255 }
    00256
    00257 //
    00258 // write4bits
    00259 void LiquidCrystal_I2C::write4bits ( uint8_t value, uint8_t mode )
    00260 {
    00261    uint8_t pinMapValue = 0;
    00262
    00263    // Map the value to LCD pin mapping
    00264    // --------------------------------
    00265    for ( uint8_t i = 0; i < 4; i++ )
    00266    {
    00267       if ( ( value & 0x1 ) == 1 )
    00268       {
    00269          pinMapValue |= _data_pins[i];
    00270       }
    00271       value = ( value >> 1 );
    00272    }
    00273
    00274    // Is it a command or data
    00275    // -----------------------
    00276    if ( mode == DATA )
    00277    {
    00278       mode = _Rs;
    00279    }
    00280
    00281    pinMapValue |= mode | _backlightStsMask;
    00282    pulseEnable ( pinMapValue );
    00283 }
    00284
    00285 //
    00286 // pulseEnable
    00287 void LiquidCrystal_I2C::pulseEnable (uint8_t data)
    00288 {
    00289    _i2cio.write (data | _En);   // En HIGH
    00290    _i2cio.write (data & ~_En);  // En LOW
    00291 }

All Classes Files Functions Variables Typedefs Enumerations Enumerator Defines