Az MCUFriend 3.5 TFT Mega illesztés paraméterei...

A zip állományol a library manager segítségével telepítendőek.
A kibontott állományok a licenszeket és a műszaki leírást tartalmazzák.

2016.01.22. TavIR

-----------------------------------------------------------------------------------------------
UTFT kijelző könyvtár
	
	A kijelző élesztési paraméterkódja (a deklaráció a setup() előtt szerepel):
	
	UTFT myGLCD(CTE32HR,38,39,40,41);
vagy 
	UTFT myGLCD(R61581,38,39,40,41);
Mindkét kijelzővezérlőt megérti a 3.5 TFT kijelző.

A kijelző forgatása az kijelző driverkönyvtárában az initlcd.h átírásával lehetséges
	LCD_Write_COM(0x36);
	LCD_Write_DATA(0x0A);
helyett
	LCD_Write_COM(0x36);
	LCD_Write_DATA(0x04); //0x0A
A 0. illetve az 1. bit átírásával a vízszintes ill függőleges tükrözés lehetséges.

-----------------------------------------------------------------------------------------------
UTOUCH
Kalibráció szükséges, mely a UTouch-Calibration futtatása adja meg és a UtouchC.h állományba íradó.

-----------------------------------------------------------------------------------------------
Pinout

Specification is: 3.5 inch TFT LCD Screen For Arduino MEGA 2560 Board
Dimension :3.5inch
Controller :R61581/CTE32HR
Resolution:  400x270
Data bits: 8 -16
Interface pin number :37 pin
Distance:1 mm

3.5 inch LCD screen interface definition (37pin):
Sequence
   Definition
1    NC
2    VDD
3    VDD
4    CS
5    RS
6    WR
7    RD
8    RESET
9    DB0
10    DB1
11    DB2
12    DB3
13    DB4
14    DB5
15    DB6
16    DB7
17    DB8
18    DB9
19    DB10
20    DB11
21    DB12
22    DB13
23   DB14
24    DB15
25    GND
26    NC
27    NC
28    NC
29    NC
30    LED-K6
31    LED-K5
32    LED-K4
33    LED-K3
34    LED-K2
35    LED-K1
36    LED-A
37   GND